EAW's PLM Series preset for EAW's MW speaker
 
MW15 Bi-amp Full Range

Application Notes:
MW15 is high-passed at 50 Hz with 18 dB Butterworth filter for 
full range operation.

"GREY" Setting: EQ slope is -1 dB per octave (constant slope) in 
half-space conditions.

Technical info:
Factory output gains assume amplifiers for each passband have the 
same voltage gain. If voltage gains of amplifiers in use do not match, 
see "LAKE_LAB.GRUPPEN README" PDF in root EAW folder for suggested trim(s).

Limiter thresholds are not engaged, and should be set by user to match amplifiers.
Attack/release times are optimized for each passband.
