Lake XP preset for ADAMSON IS7
=========================

Application Notes:
     - Default tuning for 3 to 6 cabinets stacked on 2 or 3 subs
     - Array Shaping Overlay must be recalled in a group assigned to all modules of the array
     - Linear Phase response matching all E-, S- and IS-Series Line Source and Point Source when positioned in the same distance
     - Please refer to the Adamson Amplification Chart for Maximum Cabinet Count per Amplifier

Module Routing:
     - Module out 1 - LF: Ch. 1
     - Module out 2 - HF: Ch. 2

Technical Info:
     - Fingerprint: V1.1

=======================
Designed by ADAMSON & DV2