*** TURBOSOUND BERLIN TBV Series ***
***   Constant Curvature Array   ***
____________________________________________________

TBV118L 1-WAY 80 Hz FRONT FIRING module

OUTPUTS: Ch1 = TBV118L FRONT-FIRING SUB (80 Hz LPF)

Pre-aligned for use with TBV123 in bi-amp or passive mode
when processed with "TBV123 2W FULLRANGE" or "TBV123 PASSIVE 
FULLRANGE" modules (3:1 ratio TBV123:TBV118L)

____________________________________________________

EQ OVERLAYS:

- LT COMPENSATION  

Notes:
 
1) insert LT COMPENSATION to maintain tonal balance
consistency when LT overlay is inserted in
"TBV123 2W FULLRANGE" or "TBV123 PASSIVE FULLRANGE" modules
____________________________________________________

Application Notes:

GAIN: all modules assume 35 dB amplifier gain
(for PLM this is already set and locked)

WARNING: Ensure correct routing before use.
____________________________________________________      

Please read the TBV QSG and Rigging Manual prior to use 

*** Designed by Music Group - 31 MAR 2017 ***
http://www.music-group.com/support/