Adamson's PLM Series preset for Adamson's LX12

Application Notes:
     Passive Mode
     The preset is High-passed at 120Hz
     FOH position  
     Setting for 1 cabinet per channel.

Routing:
     Ch A : 1 / 2
     Ch B : 3 / 4

Technical info:
     Amp Gain is 32 dB

Fingerprint :
     No

Designed by DV2
Pascal GUILLAUME