EAW's PLM Series preset for EAW's FRz Series speaker.
 
FR153z + FR250z Subwoofer, Bi-amp Full-Range

Application Notes:
FR153z & FR250z are crossed at 100 Hz 24 dB Linkwitz-Riley filter 
for full-range operation.

Technical info:
Factory output gains assume amplifiers for each passband have the 
same voltage gain. If voltage gains of amplifiers in use do not match, 
see "LAKE_LAB.GRUPPEN README" PDF in root EAW folder for suggested trim(s).

Limiter thresholds are not engaged, and should be set by user to match amplifiers.