EV's PLM Series preset suitable for EV's XLD281 System

Application Notes:
EV XLD281 4W Mode with 100Hz (LR24) Hi-Pass to be used with subs.

The preset is based on an electronic transfer function between EV DSP and the Lake DSP.
Output levels assume equal gain amplifiers for each passband.

EV Rev Number: Version 2.10a (Standart Preset RCM26/DX46)
Dolby Lake Rev Number: Version 1

Technical info:
* Amp Gain is 35 dB
* ISVPL threshold at 125 Vpk (LF2), 125 Vpk (LF1), 123 Vpk (HF) 
* MaxPeak limiter threshold at maximum factory value (i.e. +24 dBu-pk)
