PLM series preset for Tk Subwoofer element.

-Application Notes
     3 Tk18 per channel
     3 Tk25 per bi-amp module (Switch in dual position)
     No directionnal pattern
     Low-pass @ 70 Hz
     
-Routing
  Tk18
     Sub : 1 / 2 / 3 / 4
  Tk25
     Sub1 : 1 / 3
     Sub2 : 2 / 4

-Technical info
     Amp Gain : 32 dB

-Fingerprint file
    in further version release

--------------------------------

Designed by Kyu Systems
Romain CAHU - Thierry de CONINCK
