Lab.gruppen's PLM Series preset suitable for L-Acoustics' ARCS speaker.

Application notes:
Created for the "ARCS 3W SB118 LO" application; 
ARCS + SB118 closely coupled (80 Hz crossover), 1:1 ratio, normal HF eq.

Technical info:
* Amp Gain is 32 dB
* MaxRMS limiter threshold at +10 dBu (SUB), +8 dBu (LF), +2 dBu (HF)
* ISVPL threshold at 173.7 Vpk (SUB), 137.8 Vpk (LF), 69.1 Vpk (HF)  
* MaxPeak limiter threshold at maximum factory value (i.e. +24 dBu-pk)
  - The ISVPL threshold corresponds to a MaxPeak limiter threshold at 
    +15 dBu (SUB), +13 dBu-pk (LF), +7 dBu-pk (HF)
* When the preset is used in a PLM 10000Q, the ISVPL maximum is limited to 153.0 Vpk