*** TURBOSOUND MANCHESTER Series                             ***
***       V2.3 XP RELEASE                                    ***
*** All MODULES & OVERLAYS CREATED IN LAKE CONTROLLER V7.1.2 ***
*** All MODULES ARE CONTOUR XP FORMAT                        ***
***         README                                           ***
______________________________________________________________________________________________________
LAB GRUPPEN PLM12K44/PLM20K44 & D SERIES L DSP AMPLIFIERS ONLY - LM SERIES PROCESSORS ARE NOT SUITABLE

MC12-P 1W PASSIVE XP module for use with MS121, MS215 & MS218 subs OR stand alone
Pre-aligned for use with MSxxx XP subwoofer Modules

OUTPUTS:  CORRECT OUTPUT PATCHING XP Modules DO NOT REQUIRE MOM (module output mixing) 
instead they use the new MBL (multi-band limiter)

ISVPL profile should be set to universal
______________________________________________________________________________________________________

EQ OVERLAYS:

3 band BLEQ is set at internal crossover points of MC12-P and should be used as a 'tone/level' control. 


Notes:
 
1) do not insert ANY Array Size Compensation overlay


2) DISTANCE EQ (AirEQ) overlay not required

_______________________________________________________________________________________________________

Application Notes:

GAIN: all modules assume 35 dB amplifier gain
(for PLM / D series L this is already set and locked)

WARNING: Ensure correct routing before use 

WARNING: V1.1 & V2.3 MODULES ARE NOT DESIGNED TO BE USED TOGETHER IN THE SAME SYSTEM
_______________________________________________________________________________________________________      

Please read the MANCHESTER QSG and Rigging Manual prior to use 

All MODULES & OVERLAYS CREATED IN LAKE CONTROLLER V8.02

*** Designed by TURBOSOUND - MAR 2024 ***
http://www.turbosound.com

