Lake preset for ADAMSON M15 Passive and SPB
=============================

Application Notes:
     - FLAT EQ curve for FOH position with two coupled M15
     - Crossover: 80 Hz
     - Please refer to the Adamson Amplification Chart for Maximum Cabinet Count per Amplifier

Module Routing:
     - Module out 1 - M15: Ch. 1
     - Module out 1 - SPB: Ch. 2
     
Technical Info:
     - Fingerprint: n/a

=======================
Designed by ADAMSON & DV2