Lake FIR preset for ADAMSON E12
==========================

Application Notes:
     - Default LF compensation for 12 to 14 cabinets per array. Use Array Shaping Overlay for different array length and/or to adjust LF contour.
     - Array Shaping Overlay must be recalled in a group assigned to all modules of the array.
     - Please refer to the Adamson Amplification Chart for Maximum Cabinet Count per Amplifier

Module Routing:
     - Module out 1 - LF: Ch. 1 and 2
     - Module out 2 - MF: Ch. 3
     - Module out 3 - HF: Ch. 4

Technical Info:
     - Fingerprint: V4.0

=======================
Designed by ADAMSON & DV2