EAW's PLM Series preset for EAW's JFL speaker.

JFL210x1-3 Single-amp Full Range

Application Notes:
JFL210 is high-passed at 60 Hz with 12 dB Butterworth filter for 
full range operation. Set HF Shading switch to "Single Box" for 
1x JFL210 and "Multi Box" for 2-3x JFL210.

Technical info:
Factory output gains assume amplifiers for each passband have the 
same voltage gain. If voltage gains of amplifiers in use do not match, 
see "LAKE_LAB.GRUPPEN README" PDF in root EAW folder for suggested trim(s).

Limiter thresholds are not engaged, and should be set by user to match amplifiers.