PLM series preset for active Xo15 element.

-Application Notes
     2 way bi-amp
     Xo15 used as monitor
     Full Range preset (without subwoofer)
     Optimized for 2 Xo15 per channel

-Routing
     LF : 1 / 3
     HF : 2 / 4

-Technical info
     Amp Gain : 32 dB

-Fingerprint file
     in further version release

--------------------------------

Designed by Kyu Systems
Romain CAHU - Thierry de CONINCK
