Flashline Preset TFS-900H Low RevD

Due to current limitations of the processor, Flashline presets are currently distributed as two 2-way modules to make the complete 4 way system.

This module is for the Low/mid and Low section of the cabinet only. Load TFS-900H Hi RevC and route to outputs 3 and 4. Load  TFS-900H Low RevC and route to outputs 1 and 2.


Band gains within the module are left so that the user can adjust these +6dB & -10dB on each band to adjust the overall spectral balance of the system. 
The adjustment for the length of the line should be done using the high shelf presets, and adjustment of the band gains of the LF sections. 
If needed, a low shelf can also be added to the overall EQ for exceptionally long lines.

Input to the modules can be changed in preference order, as default this is set to AES, with the amplifier auto switching to analogue if this is not present.

Please check the Turbosound website regularly for updated settings, or sign upto the newsletter at www.turbosound.com/flashline for support email techsupport@turbosound.com

