*** TURBOSOUND LIVERPOOL TLX Series ***
***       BETA RELEASE              ***
____________________________________________________

TLX212L 1-WAY 120 Hz module

OUTPUTS: Ch1 = TLX212L Sub (120 Hz LPF)

Pre-aligned for use with TLX43 when processed with
"TLX43 2W 120 Hz" module (3:1 ratio TLX43:TLX212L)
____________________________________________________

EQ OVERLAYS:

- LT COMPENSATION  

Notes:
 
1) insert LT COMPENSATION to maintain tonal balance
consistency when LT or XLT overlays are inserted in
"TLX43 2W 120Hz" module
____________________________________________________

Application Notes:

GAIN: all modules assume 35 dB amplifier gain
(for PLM this is already set and locked)

WARNING: Ensure correct routing before use.
____________________________________________________      

Please read the TLX QSG and Rigging Manual prior to use 

*** Designed by Music Group - 16 MAR 2017 ***
http://www.music-group.com/support/