EV's PLM Series preset suitable for EV's XLC System

Application Notes:
EV XLC118 to be used with XLC127DVX and XLC907DVX (34Hz - 80Hz)

The preset is based on an electronic transfer function between EV DSP and the Lake DSP.
Output levels assume equal gain amplifiers for each passband.
The sub to top ratio is set to 3/2 (i.e. 3x127's with 2x118's).
Subwoofers are time-aligned and level adjusted to be flown in the 
same array, or in an array directly next to the main XLC hang.
Output levels and delay settings will need to change if XLC118 is 
used with systems other than XLC.

EV Rev Number: Version 2 (Standart Preset RCM26)
Dolby Lake Rev Number: Version 1

Technical info:
* Amp Gain is 35 dB
* ISVPL threshold at 130 Vpk (SUB) 
* MaxPeak limiter threshold at maximum factory value (i.e. +24 dBu-pk)