*** TURBOSOUND MANCHESTER Series                             ***
***       V2.3 XP RELEASE                                    ***
*** All MODULES & OVERLAYS CREATED IN LAKE CONTROLLER V7.1.2 ***
*** All MODULES ARE CONTOUR XP FORMAT                        ***
***         README                                           ***
______________________________________________________________________________________________________
LAB GRUPPEN PLM12K44/PLM20K44 & D SERIES L DSP AMPLIFIERS ONLY - LM SERIES PROCESSORS ARE NOT SUITABLE

MV212 2W module for use with MS121, MS215 & MS218 subs
Pre-aligned for use with MSxxx XP subwoofer Modules

OUTPUTS:  CORRECT OUTPUT PATCHING XP Modules DO NOT REQUIRE MOM (module output mixing) 
instead they use the new MBL (multi-band limiter)

ISVPL profile should be set to Sub/LF for 12" LF and universal for MF & HF
______________________________________________________________________________________________________

EQ OVERLAYS:

SEE SEPARATE "Array Size Comp" & "Distance EQ" Folders 
FOR ARRAY OPTIMISATION OF LINE LENGHT AND DISTANCE EQ (ZONAL/THROW HF CONTROL)

Notes:
 
1) do not insert more than one Array Size Compensation overlay at the same time, 
whole array should have same overlay inserted

2) each ZONE of elements within the Array uses the nearest DISTANCE EQ (AirEQ) overlay 

_______________________________________________________________________________________________________

Application Notes:

GAIN: all modules assume 35 dB amplifier gain
(for PLM / D series L this is already set and locked)

WARNING: Ensure correct routing before use 

WARNING: V1.1 & V2.3 MODULES ARE NOT DESIGNED TO BE USED TOGETHER IN THE SAME SYSTEM
_______________________________________________________________________________________________________      

Please read the MANCHESTER QSG and Rigging Manual prior to use 

All MODULES & OVERLAYS CREATED IN LAKE CONTROLLER V8.02

*** Designed by TURBOSOUND - MAR 2024 ***
http://www.turbosound.com
