EAW's PLM Series preset for EAW's JFL speaker.

JFL210x4-6 Single-amp Full Range

Application Notes:
JFL210 is high-passed at 60 Hz with 12 dB Butterworth filter for 
full range operation. Use HF Shading switches to taper HF response 
throughout an array. Recommended top-to-bottom progressions are:

* 4x JFL210: Long Throw, Multi Box, Multi Box, Single Box
* 5x JFL210: Long Throw, Long Throw, Multi Box, Multi Box, Single Box
* 6x JFL210: Long Throw, Long Throw, Multi Box, Multi Box, Multi Box, Single Box

Technical info:
Factory output gains assume amplifiers for each passband have the 
same voltage gain. If voltage gains of amplifiers in use do not match, 
see "LAKE_LAB.GRUPPEN README" PDF in root EAW folder for suggested trim(s).

Limiter thresholds are not engaged, and should be set by user to match amplifiers.