Lab.gruppen's PLM Series preset suitable for L-Acoustics' SYVA and SYVA Low with optional SYVA Sub. v5.8

Application notes:
The module file is a 2- or 3-way configuration, high-passed at 200 Hz.
The SYVA filter is FIR and on output 3. Sub is on output 1 and LF is on output 2
Delay range is 0 - 20ms for all enclosures for flexible placement

Technical info:
* Amp Gain is 35 dB
* MaxRMS limiter threshold at +3.5 dBu (SYVA and SYVA Low), +4 dBu (Sub)
* ISVPL threshold at 140 Vpk (SYVA), 150 Vpk (Sub)
* MaxPeak limiter threshold at maximum factory value (i.e. +24 dBu-pk)
  - The ISVPL threshold corresponds to a MaxPeak limiter threshold at 
    +10 dBu-pk (SYVA), +12 dBu-pk (Sub)

