TURBOSOUND's NuQ122 Bi-Amped FIR preset + NuQ115B SUB

This preset is for FOH applications.

As this is an FIR preset, two modules of processing are required (A+B or C+D) and this preset is not compatible with LM series processors.

Application notes:

Channel 1 = NuQ115B SUB
Channel 2 = NuQ122 LF
Channel 3 = NuQ122 HF

LF is Full Range, HPF at 50Hz

Total Processor Delay is 6.31ms

Technical info:
* Amp Gain is 35 dB
* MaxRMS limiter threshold at 3 dBu (SUB), 2 dBu (LF), -9.3 dBu (HF)
* MaxPeak limiter threshold at 9 dBu (SUB), 8 dBu (LF), -3.3 dBu (HF)
* ISVPL threshold at 89 Vpk (SUB), 80 Vpk (LF), 22 Vpk (HF)  

**Designed by MUSIC TRIBE BRANDS Ltd 2019**
