PLM Series preset for Kryter12 line source element.

-Application Notes
     3 way Quad-amp
     Full Range preset (without subwoofer)
     Optimized for 3 Kryter12 elements
     in parallel per channel

-Routing
     LF1 : 1
     LF2 : 2
     MF  : 3
     HF  : 4

-Technical info
     Amp Gain :  32 dB

-Fingerprint file
    in further version release

--------------------------------

Designed by Kyu Systems
Romain CAHU - Thierry de CONINCK
