TURBOSOUND's NuQ82 Full Range FIR preset + NuQ115B or NuQ118B SUB's

This preset is for FOH applications.

As this is an FIR preset, two modules of processing are required (A+B or C+D) and this preset is not compatible with LM series processors.

Application notes:

Channel 1 = NuQ118B SUB
Channel 2 = NuQ115B SUB
Channel 3 = NuQ82 Full Range

HPF on NuQ82 channel is at 50Hz

Total Processor Delay is 6.35ms

Technical info:
* Amp Gain is 35 dB
* MaxRMS limiter threshold at 3.7 dBu (NuQ118B), 3 dBu (NuQ115B), 1 dBu (NuQ82)
* MaxPeak limiter threshold at 9.7 dBu (NuQ118B), 9 dBu (NuQ115B), 7 dBu (NuQ82)
* ISVPL threshold at 100 Vpk (NuQ118B), 89 Vpk (NuQ115B), 69 Vpk (NuQ82)  

**Designed by MUSIC TRIBE BRANDS Ltd 2019**
