PLM Series preset for Juno line source element.

-Application Notes
     3 way bi-amp
     High-pass @ 70 Hz
     Optimized for 4 Juno10 elements
     in parallel per channel

-Routing
     LF   : 1 / 3
     MFHF : 2 / 4

-Technical info
     Amp Gain :  32 dB

-Fingerprint file
    in further version release

--------------------------------

Designed by Kyu Systems
Romain CAHU - Thierry de CONINCK
