Adamson's PLM Series preset for Adamson's SpekTrix Sub speaker.

Application Notes:
     The preset is low-passed at 160 Hz and High-passed at 60Hz 24dB Linkwitz Riley.
     Maximum of 2 cabinets in parallel per channel.
     Spek-Trix 5W mode to be used with Infra Sub.

Routing:
     SUB : 1

Technical info:
     Amp Gain is 32 dB

Fingerprint:
     No

Designed by DV2
Pascal GUILLAUME