*** Tannoy VX Series PASSIVE ***
___________________________________________________________________

PLM & LM Series preset for Tannoy VX Series
Products utilised in Passive mode


Dual: VX5.2, VX6, VX8, VX8.2, VX12
HP: VX12HP, VX15HP
Q-Centric: VX12Q, VX12.2Q, VX15Q, 
___________________________________________________________________

Application Notes:

This 3 AUX module has 3 Proccesed outputs:

1 = FLAT : Fullrange Settings
2 = CUT : 80Hz LF Cut (For use either standalone or with Sub)
3 = SUB : Matched Sub output for use with the above CUT output

This module can be used in combination with VSX Sub Module Files
should a different combination other than the one 
supplied be required.
___________________________________________________________________

Routing:

Any channel can be routed to the required output from this module.
WARNING:: Ensure correct routing before use.
___________________________________________________________________    

Technical info:
	
Amp Gain is 33 dB
(This is to align better with Lab.gruppen IPD Series)
If using with IPD & PLM please ensure the IPD is delayed by 1.16 mS
___________________________________________________________________

Fingerprint :	

No
___________________________________________________________________

*** Designed by TCGROUP AET ***

::: Thomas Vestergaard :::
