Lab.gruppen's PLM Series preset suitable for JBL's VT4880 speaker.

Application notes:
Designed to be used together with "VT4888 60 for VT4880" preset.

The preset is designed for a subwoofer application, low-passed 
at 60 Hz. Default settings for user gain (+10 dB) and delay (5.00 ms) 
can be edited to align the cabinet with the system.

Please be aware of the routing limitations regarding input gain, 
input eq and input delay when using the third output.

Technical info:
* Amp Gain is 32 dB
* MaxRMS limiter threshold at +11 dBu (SUB)
* ISVPL threshold at 154.8 Vpk (SUB)  
* MaxPeak limiter threshold at maximum factory value (i.e. +24 dBu-pk)
  - The ISVPL threshold corresponds to a MaxPeak limiter threshold at 
    +14 dBu-pk (SUB)
* When the preset is used in a PLM 10000Q, the ISVPL maximum is limited to 153.0 Vpk
* To emulate 26 dB Amp Gain - set input gain to -6 dB

Fingerprint info:
VT4880 v1.0b1 (2 ch)