*** Tannoy VX Series BI-AMP MODE MONITOR ***
___________________________________________

PLM & LM Series preset for Tannoy VX Series
Products utilised in Bi-Amplification MONITOR mode

HP: VX12HP, VX15HP
 
___________________________________________

Application Notes:

This Module has 3 Processed outputs:

1 = LF : Low Frequency Driver
2 = HF : High Frequency Driver Compliment
3 = SUB : Matched Sub output for use with the above

This is a Tailored module file for Stage Monitor and Foldback applications and is designed to offer optimal
performance in these applications.
___________________________________________

Routing:

Any channel can be routed to the required output from this module.
WARNING:: Ensure correct routing before use.
___________________________________________      

Technical info:
	
Amp Gain is 33 dB
(This is to align better with Lab.gruppen IPD Series)
If using with IPD & PLM please ensure the IPD is delayed by 1.16 mS
___________________________________________

Fingerprint :	

No
___________________________________________

*** Designed by TCGROUP AET ***

::: Thomas Vestergaard :::
