FA22-60
Dual 12 inch Coaxial Loudspeaker (Bi-amp)
60 x 45 degree nominal beamwidth

Application Notes:
Pre-Out EQ tab has user-adjustable high pass filter. Set it no lower than 40 Hz, 24 dB Linkwitz-Riley for full range operation.

Technical info:
* Amplifier Gain is set to 32 dB.
* Factory ISVPL Speaker Thresholds and MaxRMS Limiter Thresholds are engaged.