*** TURBOSOUND BERLIN TBV Series ***
***   Constant Curvature Array   ***
____________________________________________________

TBV123 PASSIVE 1-WAY + TBV118L 1-WAY + TBV118L CARDIOID 1-WAY

OUTPUTS: Ch1=TBV123
	 Ch2=TBV118L 
	 Ch3=TBV118L CARDIOID

XOVER AT 120 Hz
____________________________________________________

EQ OVERLAYS:
Nominal flat single enclosure response (EQ overlays bypassed)

- LT COMPENSATION  
- 2 BOX (nominal flat response for 2x TBV123)
- 3 BOX (nominal flat response for 3x TBV123)
- Long Throw (6 dB HF / 4 dB LF shelving applied)
- BLEQ (Band Level EQ) - adjust to obtain desired tonal balance

Notes:
 
1) insert LT COMPENSATION to maintain tonal balance
consistency when LT overlay is inserted
____________________________________________________

Application Notes:

GAIN: all modules assume 35 dB amplifier gain
(for PLM this is already set and locked)

WARNING: Ensure correct routing before use.
____________________________________________________      

Please read the TBV QSG and Rigging Manual prior to use 

*** Designed by Music Group - 31 MAR 2017 ***
http://www.music-group.com/support/