Adamson's PLM Series preset for Adamson's Y10K and Spek-trix

Application Notes:
     This module was designed to be used as a supermodule
     Y10K : LF = Kevlar Cone Driver 16Ohms
     The preset is high-passed at 90 Hz 

Routing:
     Y10K LF : 1 & 2
     Y10K MF : 3
     Y10K HF : 4
     SPK LF : 2
     SPK MF : 3
     SPK HF : 4

Technical info:
     Amp Gain is 32 dB

Fingerprint:
     No

Designed by DV2
Pascal GUILLAUME
     