*** TURBOSOUND LIVERPOOL TLX Series ***
***       BETA RELEASE              ***
____________________________________________________

TLX84 + TLX215L 3-WAY 80 Hz module

OUTPUTS: Ch1=SUB (polarity inverted); Ch2=LF; Ch3=HF

TLX84 pre-aligned for use with TLX215L subwoofers at
3:1 ratio but other TURBOSOUND subs can be used
____________________________________________________

EQ OVERLAYS:

- Long Throw (LT)  
- Extra Long Throw (XLT)

Notes:
 
1) do not insert LT and XLT overlays at the same time

2) for single enclosure short throw applications bypass LT 
and XLT overlays to obtain nominal flat response

3) Use "Array Size Compensation" and "BLEQ" Band Level EQ
overlays to achieve the desired tonal balance
____________________________________________________

Application Notes:

GAIN: all modules assume 35 dB amplifier gain
(for PLM this is already set and locked)

WARNING: Ensure correct routing before use.
____________________________________________________      

Please read the TLX QSG and Rigging Manual prior to use 

*** Designed by Music Group - 16 MAR 2017 ***
http://www.music-group.com/support/