Lake XP preset for ADAMSON IS10
=========================

Application Notes:
     - Default tuning for Lip Fill application
     - Linear Phase response matching all E-, S- and IS-Series Line Source and Point Source when positioned in the same distance
     - Please refer to the Adamson Amplification Chart for Maximum Cabinet Count per Amplifier

Module Routing:
     - Module out 1 - LF: Ch. 3 / 1 with pin swap cable
     - Module out 2 - HF: Ch. 4 / 2 with pin swap cable

Technical Info:
     - Fingerprint: V3.0

=======================
Designed by ADAMSON & DV2

