PLM series preset for Kryter10 line source element.

-Application Notes
     3 way bi-amp
     Full Range preset (without subwoofer)
     Optimized for 4 Kryter10 elements
     in parallel per channel

-Routing
     LF   :  1 / 3
     MFHF :  2 / 4

-Technical info
     Amp Gain : 32 dB

-Fingerprint file
    in further version release

--------------------------------

Designed by Kyu Systems
Romain CAHU - Thierry de CONINCK
