Lake preset for ADAMSON IS5c
========================

Application Notes:
     - Low cut
     - Recommended to use with 100 Hz Subwoofer presets
     - Conventional Crossover
     - Add 6.4 ms of delay for high frequency phase alignment with linear phase presets in the same distance 
     - Please refer to the Adamson Amplification Chart for Maximum Cabinet Count per Amplifier


Module Routing:
     - Module out 1 - FR: Ch. 1

Technical Info:
     - Fingerprint: n/a

=======================
Designed by ADAMSON & DV2