EV's PLM Series preset suitable for EV's XLD/XLE System.

Application Notes:
EV X-Sub to be used with XLD281 and XLE181 sytems (33Hz - 100Hz)

The preset is based on an electronic transfer function between EV DSP and the Lake DSP.
Output levels assume equal gain amplifiers for each passband.


EV Rev Number: Version 1.10a (Standart Preset)
Dolby Lake Rev Number: Version 1

Technical info:
* Amp Gain is 35 dB
* ISVPL threshold at 130 Vpk (SUB) 
* MaxPeak limiter threshold at maximum factory value (i.e. +24 dBu-pk)
