Lab.gruppen's PLM Series preset suitable for JBL's VTX A8 speaker, V0.1 Rel 1.1.1

Application notes:
The preset is designed for use in arrays, Full Range
The filter is FIR and output 3 is MF+HF, output 2 LF and output 1 is a B18 sub.
Outputs can be dealy adjusted 0 - 20 ms to support Sub placements. LF and HMF shall be the same setting to perserve the factory alignment.
Totallatency is 6.35 ms to match system performance.

Technical info:
* Amp Gain is 35 dB
* MaxRMS limiter threshold at +7 dBu (Sub), +4 dBu (LF) and +1 dBu (HMF)
* ISVPL thresholdat 180 Vpk (SUB), 160 Vpk (LF) and 160 Vpk (HMF) 
* MaxPeak limiter threshold at maximum factory value (i.e. +24 dBu-pk)
 
