Turbosound's PLM Series FIR preset suitable for Turbosound's TFA-600H speaker.

Application notes:
The module file is created for a tri-amped cabinet with a HF shelving filter
which can be manipulated by the user. This module file is designed for use either 
when the loudspeaker is used as a single point source or for extremely 
near-field applications for up to 3 TFA-600H units.
If using more than 3 cabinets, then increase the high shelf on the EQ page which is currently set to 0dB gain. 
Or use the preset manager to load preset files into the device.

When used in combination with subwoofers TSW218 or TFA-600L, the preset can be used together
with a "TSW218 for Flex FIR RevA" or "TFA-600L for Flex FIR RevA" preset.

Technical info:
* Amp Gain is 35.7 dB (LF), 26 dB (MF), 26 dB (HF)
* MaxRMS limiter threshold at +3.3 dBu (LF), +6 dBu (MF), +3 dBu (HF)
* ISVPL threshold at 97.7 Vpk (LF), 61.6 Vpk (MF), 61.6 Vpk (HF)  
* MaxPeak limiter threshold at maximum factory value (i.e. +24 dBu-pk)
  - The ISVPL threshold corresponds to a MaxPeak limiter threshold at 
    +6.3 dBu-pk (LF), +12 dBu-pk (MF), +12 dBu-pk (HF)