Adamson's PLM Series preset for Adamson's SpekTrix Sub speaker.

Application Notes:
     The preset is low-passed at 110 Hz 
     Maximum of 2 cabinets in parallel per channel.

Routing:
     SUB : 1

Technical info:
     Amp Gain is 32 dB

Fingerprint:
     No

Designed by DV2
Pascal GUILLAUME