Adamson's PLM Series preset for Adamson's 12MX

Application Notes:
     Active Mode
     Wedge monitor position 

Routing:
    LF : 1 / 3
    HF : 2 / 4

Technical info:
     Amp Gain is 32 dB

Fingerprint :
     No

Designed by DV2
Pascal GUILLAUME