Lake preset for MDC-1 SUB

Application Notes:
     The preset is low-passed at 100 Hz

Routing MDC1
     SUB : 1+1-
     OUTPUT to crosslink SUB2 : 2 

Technical info:
     Amp Gain is 32 dB

Fingerprint: 
     No

Designed by DV2
Pascal GUILLAUME