EV's PLM Series preset suitable for EV's XLC System.

Application Notes:
EV XLC-907DVX 4w Mode with 80Hz (LR24) Hi-Pass to be used without subs.

The preset is based on an electronic transfer function betwwen EV DSP and the Lake DSP.
Output levels assume equal gain amplifiers for each passband.
The XLC127DVX and XLC907DVX V2.0 presets are time-aligned to 
allow multi-pattern array creation.

EV Rev Number: Version 2.0 (Standart Preset IIR/RCM26)
Dolby Lake Rev Number: Version 1.0

Technical info:
* Amp Gain is 35 dB
* ISVPL threshold at 150 Vpk (LF), 109 Vpk (MF), 84 Vpk (HF) 
* MaxPeak limiter threshold at maximum factory value (i.e. +24 dBu-pk)