*** TURBOSOUND BERLIN TBV Series ***
***   Constant Curvature Array   ***
____________________________________________________

TBV123 2W BI-AMP + TBV118L 3-WAY 120 Hz module

OUTPUTS: Ch1=TBV118L 120 Hz LPF
	 Ch2=TBV123 LF 120 Hz HPF
	 Ch3=TBV123 HF

TBV123 pre-aligned for use with TBV118L front-firing subwoofers 
at 3:1 ratio but other TURBOSOUND subs can be used
____________________________________________________

EQ OVERLAYS:

- 2 BOX (nominal flat response for 2x TBV123)
- 3 BOX (nominal flat response for 3x TBV123)
- Long Throw (6 dB HF / 4 dB LF shelving applied)
- BLEQ (Band Level EQ) - adjust to obtain desired tonal balance
____________________________________________________

Application Notes:

GAIN: all modules assume 35 dB amplifier gain
(for PLM this is already set and locked)

WARNING: Ensure correct routing before use.
____________________________________________________      

Please read the TBV QSG and Rigging Manual prior to use 

*** Designed by Music Group - 31 MAR 2017 ***
http://www.music-group.com/support/
