Adamson's PLM Series preset for Adamson's Y18 speaker.

Application Notes:
     OUTDOOR
     The preset is high-passed at 60 Hz
     Maximum 2 cabinets in parallel per amplifier.

Routing:
     LF : 1 & 2
     MF : 3
     HF : 4

Technical info:
     Amp Gain is 32 dB

Fingerprint: 
     Y18 v1.0b1 BETA

Designed by DV2
Pascal GUILLAUME