EV's PLM Series preset suitable for EV's X-LINE System.

Application Notes:
EV XVLS 3w Mode with 50Hz (BU24) Hi-Pass to be used without subs

The preset is based on an electronic transfer function between EV DSP and the Lake DSP.
Output levels assume equal gain amplifiers for each passband.

EV Rev Number: Version 4 (Standart Preset IIR/RCM26)
Dolby Lake Rev Number: Version 1.0

Technical info:
* Amp Gain is 35 dB
* ISVPL threshold at 130 Vpk (LF), 110 Vpk (MF), 84 Vpk (HF) 
* MaxPeak limiter threshold at maximum factory value (i.e. +24 dBu-pk)
