PLM Series preset for MDC-3 SUB

Application Notes:
     The preset is low-passed at 60 Hz
     Maximum of 1 cabinet per channel.

Routing MDC3
     SUB : 1
     OUTPUT to crosslink SUB2 : 2 

Technical info:
     Amp Gain is 32 dB

Fingerprint: 
     No

Designed by DV2
Pascal GUILLAUME