EAW's PLM Series preset for EAW's KF speaker
 
KF761 Array Tri-amp Full Range

Application Notes:
KF761 is high-passed at 40 Hz with 24 dB Butterworth filter for 
full range operation.

Technical info:
Factory output gains assume amplifiers for each passband have the 
same voltage gain. If voltage gains of amplifiers in use do not match, 
see "LAKE_LAB.GRUPPEN README" PDF in root EAW folder for suggested trim(s).

Limiter thresholds are not engaged, and should be set by user to match amplifiers.

Fingerprint:  KF761 v1.0b BETA
Beta fingerprints may produce incorrect results.