Adamson's PLM Series preset for Adamson's B118.

Application Notes:
     The preset is low-passed at 120 Hz 
     Maximum of 4 cabinets per Channel.

Routing:
     B118 : 1+ 1-

Technical info:
     Amp Gain is 32 dB

Fingerprint: 
     No

Designed by DV2
Pascal GUILLAUME