EAW's PLM Series preset for EAW's AX Series speaker.
 
AX344 Single-amp w/ Sub High-Pass Filter

Application Notes:
AX344 is high-passed at 80 Hz with 24 dB Linkwitz-Riley filter for 
use with subwoofer.

Technical info:
Factory output gains assume amplifiers for each passband have the 
same voltage gain. If voltage gains of amplifiers in use do not match, 
see "LAKE_LAB.GRUPPEN README" PDF in root EAW folder for suggested trim(s).

Limiter thresholds are not engaged, and should be set by user to match amplifiers.