Lab.gruppen's PLM Series preset suitable for L-Acoustics' dV-SUB speaker.

Application notes:
1+1 module created for the "dV-SUB 80 Hz" application. If used together with dV-DOSC; 
then use "dV-DOSC 80 Hz LO/HI" preset. Each of the 2 identical subwoofer channels has 
a separate input mixer to allow for a Left and Right subwoofer that only uses one module.

Please be aware of the routing limitations regarding input gain, 
input eq and input delay when using the third output.

Technical info:
* Amp Gain is 32 dB
* MaxRMS limiter threshold at +8 dBu (SUB)
* ISVPL threshold at 137.8 Vpk (SUB)  
* MaxPeak limiter threshold at maximum factory value (i.e. +24 dBu-pk)
  - The ISVPL threshold corresponds to a MaxPeak limiter threshold at 
    +13 dBu-pk (SUB)

Fingerprint info:
dV-SUB v1.0 beta1