*** Turbosound FLASHLINE MONITORS TFM Series ***
____________________________________________________

PLM & LM series modules:

TFM122M, TFM152M, and with sub settings have TMS118B but
this can be substituted by other subs
____________________________________________________

Application Notes:

GAIN: all modules assume amplifier gain is 35dB.
For PLM this is already set and locked.
____________________________________________________

These modules have 1, 2 or 3 processed output channels:
FR = Full Range (1 Channel)
FR + Sub = Full Range and Subwoofer (2 Channels)
Bi-amp Full Range (2 Channels)
Bi-amp + Sub (3 Channels)
____________________________________________________

EQ Overlay:

ALL modules have an additional version with
a 'VOX' overlay. This is to give a simple microphone
eq that should give good performance for standard
microphone types
____________________________________________________

Routing:

Any channel can be routed to the required output
from these modules.

For monitor applications requiring a separate mix to
Full range and sub channels. Load the modules twice
mute and route the inputs an outputs accordingly.

WARNING: Ensure correct routing before use.
____________________________________________________      
Please read the QSG prior to use and for more information.

*** Designed by Music Group ***

::: Andrew Pardoe 16/05/10 :::